#include "VL6180.h"

#include "mbed.h"

VL6180 rf(I2C\_SDA, I2C\_SCL); //I2C sda and scl

int main()

{

float reading;

while(1) {

reading = rf.read();

printf("Read %4.1f cm\n", reading);

wait\_ms(500);

}

}

