#include "mbed.h"

Ticker toggle\_led\_ticker;

DigitalOut led1(LED1);

void toggle\_led()

{

led1 = !led1;

}

int main()

{

// Init the ticker with the address of the function (toggle\_led) to be attached and the interval (100 ms)

toggle\_led\_ticker.attach(&toggle\_led, 0.1);

while (true) {

// Do other things...

}

}

